# Do not edit.
# Any changes will be lost on upgrade.

description=Hostapd (template based)
radiusDisconnect=disconnect
acceptVlan = <<EOT
Tunnel-Medium-Type  = 6
Tunnel-Type = 13
Tunnel-Private-Group-Id = $vlan
EOT
acceptRole = <<EOT
Filter-Id = $role
EOT
reject=<<EOT
Reply-Message = This node is not allowed to use this service
EOT
disconnect=<<EOT
Calling-Station-Id = ${macToEUI48($mac)}
NAS-IP-Address = $disconnectIp
EOT
