<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;"># Do not edit.
# Any changes will be lost on upgrade.
acceptVlan= &lt;&lt;EOT
Tunnel-Type = 13
Tunnel-Medium-Type = 6
Tunnel-Private-Group-Id = $vlan
EOT
acceptRole=
disconnect= &lt;&lt;EOT
Calling-Station-Id = ${macToEUI48($mac)}
NAS-IP-Address = $disconnectIp
EOT
description=AeroHive - Extreme Access Point
voip=
radiusDisconnect=disconnect
reject=Reply-Message = This node is not allowed to use this service
coa=
</pre></body></html>